For a complete list of states you may refer to the s-parameters available on the AM3152 product page for the 0.4 GHz to 8 GHz section. For additional s-parameters in the 20 MHz to 500 MHz section you may refer to the AM3150 and AM3155 data-sets available on their individual product pages, then cascade with an AM3152 bypass on the input and the output. 